Force Load program - to load bad tapes into memory and display on screen.
Mike Herbach 3-26-78.

This is a program to allow the loading of any source (program) tape into
memory regardless of any bugs that would normally cause loading errors.
Just give the program the address of the start of text buffer and start
the tape recorder. You must push the system reset button to stop the
program and then edit the garbage in the first and last lines and any
other errors you find. When a semicolon (;) is seen the program goes into
a routine to ignore it and omit the sumcheck and program name info on the
tape. The text is displayed on the screen with 40 stops for readability
and there is a little garbage left on the screen after a semicolon is seen
but the memory is clean.

